*** TS8546L S-Parameter Data ***

------

Useful resources:
	TagoreTech Inc. https://www.tagoretech.com/

------

Matching network

TS8546 wideband match
Component	Part Number	Description
T0a		5.2 mm		PCB transmission line length (edge of switch to center of cap)
C0a		0603N0R4BW251	Ceramic capacitor, 0.4 pF, 250V, ± 0.1pF
T1a		4.5 mm		PCB transmission line length (edge of switch to center of cap)
C1a		0603N0R2BW251	Ceramic capacitor, 0.2 pF, 250V, ± 0.1pF
T2a		4.5 mm		PCB transmission line length (edge of switch to center of cap)
C2a		0603N0R2BW251	Ceramic capacitor, 0.2 pF, 250V, ± 0.1pF
T3a		4.5 mm		PCB transmission line length (edge of switch to center of cap)
C3a		0603N0R2BW251	Ceramic capacitor, 0.2 pF, 250V, ± 0.1pF
T4a		4.5 mm		PCB transmission line length (edge of switch to center of cap)
C4a		0603N0R2BW251	Ceramic capacitor, 0.2 pF, 250V, ± 0.1pF


Please consult the TS8546L datasheet on the TagoreTech website.

------

S5P file format.
	Port 1 - Common port.
	Port 2 - RF1 port.
	Port 3 - RF2 port.
	Port 4 - RF3 port.
	Port 5 - RF4 port.


------

For more details and additional support, please consult the TagoreTech website.